Nathan Upperman

Xi Li

Chris Andrews

Cascode Current Mirror Rev2

**Overview**

The cascode current mirror has an improved output resistance compared to the source degenerated current mirror, but at the cost of reduced headroom. The minimum operating range for the input voltage to the cascade current mirror is 2(Vtn + Vov). The minimum operating voltage for the output port is Vtn + 2Vov. Using the 50nm cmosedu\_models library gives a VTHO = 0.22V spice parameter for the threshold voltage. This means that the current mirror can function with input and output voltages of as low as 0.44V and 0.22V, but only with a negligible current of several microamps. Our Ibias current is chosen as 50uA which the cascade current source cannot sustain with a vdd = 1V operating rail.




Figure Cascode Current Mirror showing Resistive current source. Note that *v1* is the input voltage of the current mirror and *vout* is the output voltage of the current mirror that determine the operating range of the cascade current mirror. Q5 is the common source amplifier.

The parameters that we are using for this simulation are:

Vdd = 1V

Ibias= 50uA

W/L = 5

VTHO = 0.22V

The cmosedu\_models.txt spice file is a level 54 spice simulation meaning that we cannot readily get the for the circuit. Instead we bias the circuit properly so that all the transistors are in saturation, then produce the signal on the waveform.

which is not remotely far from the 280 listed for the 45nm CMOS process in table 1.5. What does this mean for the Ibias and input voltage of our circuit?

Suppose Ibias = 50uA. Then 0.47V .

Then the input voltage would be 2(Vtn + Vov) = 2(.22 + .47) = 1.38V > Vdd = 1V. If we put a 50uA ideal current source for Ibias, we show the input voltage to be simulated at 1.6V. In other words, the cascade current source lacks the headroom to source or sink a significant current with a low supply rail. For the sake of comparison, let’s increase the supply rail to 1.8V and sweep the output node vout to produce a graph that shows the operation of the cascade current mirror.

If we define the current mirror to be in operation when Iout = Ibias +- 10%, then

Vout minimum = 500mV with Ibias supplied by an ideal current source. When using a resistive current source (R = 4kΩ for Ibias = 50uA) and a 1.8V supply rail, Vout minimum = 550mV.

For the PMOS common source amplifier, it is required that *vin* – *vdd* < vtho = -.22V. Then the operating range of the current mirror extends up to *vdd*  - 0.22V.

The range of *v1* the input voltage is essentially 0, because the *v1* is fixed by the bias current.

Meaning that any change in the input voltage *v1* will necessarily change the and thus change the bias current. With the 4kΩ resistor and *a* 1.8V supply rail, *v1* = 1.64V.

This then is what we want to see in improved versions of the current mirror:

1. Minimize voltage supply.
2. Minimize the output voltage *vout* and input voltage *v1* of the current mirror to maximize range of operation.




Figure DC sweep of the output voltage *vout* showing the current mirror falling off when *vout* approaches Vtn + 2Vov = 550mV




Figure The cascade current can operate at lower vout provided that the bias current is sufficiently small. The output current I(Mq4) (blue) falls off as Vout drops below 250mV. This is the case where Vov Then Vtn + 2Vov Vtn = 220mV. Note that this result is from a 5uA ideal current source.

Discussion: Why does the wide-swing offer the best tradeoff? Why is low Vout current mirror important in circuits with steadily declining voltage supply overhead? What are the tradeoffs between Wide-swing rev0 and rev1? What would a current mirror normally interface with? What is the frequency response of the IM with a common-source amp at the output?

Cascode Current Mirror.




Figure Cascode Current Mirror

The most important parameters of the current mirror are the minimum output voltage Vout, the output resistance **Rout**.

Sweeping Vout from 5V to 0V, it is clear that the current mirror decays once Q2 and Q4 leave saturation.

Note that where

=.6696 + .6()

= .736V




Figure Vout vs. Id4. Note that current falls at approximately .7V

The output resistance of the cascade current mirror is where




Figure Rout = V(vout)/Id(Mq4) . Note that Rout is heavily dependent upon biasing. At the onset of saturation, Vout = 1V, Rout = 20kΩ.

For frequency and gain analysis, we use the current mirror to supply the bias current for a PMOS common source amp.




Figure Common Source amp stage (PMOS) to test frequency response of cascode mirror.

Id/vin = 140u s ->

Rds = 1/lambda \*Id = 1

\* BSIM3 models for AMI Semiconductor's C5 process

\*

\* Don't forget the .options scale=300nm if using drawn lengths

\* and the MOSIS SUBM design rules

\*

\* 2<Ldrawn<500 10<Wdrawn<10000 Vdd=5V

\* Note minimum L is 0.6 um while minimum W is 3 um

\* Change to level=49 when using HSPICE or SmartSpice

.MODEL NMOS NMOS ( LEVEL = 8

+VERSION = 3.1 TNOM = 27 TOX = 1.39E-8

+XJ = 1.5E-7 NCH = 1.7E17 VTH0 = 0.6696061

+K1 = 0.8351612 K2 = -0.0839158 K3 = 23.1023856

+K3B = -7.6841108 W0 = 1E-8 NLX = 1E-9

+DVT0W = 0 DVT1W = 0 DVT2W = 0

+DVT0 = 2.9047241 DVT1 = 0.4302695 DVT2 = -0.134857

+U0 = 458.439679 UA = 1E-13 UB = 1.485499E-18

+UC = 1.629939E-11 VSAT = 1.643993E5 A0 = 0.6103537

+AGS = 0.1194608 B0 = 2.674756E-6 B1 = 5E-6

+KETA = -2.640681E-3 A1 = 8.219585E-5 A2 = 0.3564792

+RDSW = 1.387108E3 PRWG = 0.0299916 PRWB = 0.0363981

+WR = 1 WINT = 2.472348E-7 LINT = 3.597605E-8

+XL = 0 XW = 0 DWG = -1.287163E-8

+DWB = 5.306586E-8 VOFF = 0 NFACTOR = 0.8365585

+CIT = 0 CDSC = 2.4E-4 CDSCD = 0

+CDSCB = 0 ETA0 = 0.0246738 ETAB = -1.406123E-3

+DSUB = 0.2543458 PCLM = 2.5945188 PDIBLC1 = -0.4282336

+PDIBLC2 = 2.311743E-3 PDIBLCB = -0.0272914 DROUT = 0.7283566

+PSCBE1 = 5.598623E8 PSCBE2 = 5.461645E-5 PVAG = 0

+DELTA = 0.01 RSH = 81.8 MOBMOD = 1

+PRT = 8.621 UTE = -1 KT1 = -0.2501

+KT1L = -2.58E-9 KT2 = 0 UA1 = 5.4E-10

+UB1 = -4.8E-19 UC1 = -7.5E-11 AT = 1E5

+WL = 0 WLN = 1 WW = 0

+WWN = 1 WWL = 0 LL = 0

+LLN = 1 LW = 0 LWN = 1

+LWL = 0 CAPMOD = 2 XPART = 0.5

+CGDO = 2E-10 CGSO = 2E-10 CGBO = 1E-9

+CJ = 4.197772E-4 PB = 0.99 MJ = 0.4515044

+CJSW = 3.242724E-10 PBSW = 0.1 MJSW = 0.1153991

+CJSWG = 1.64E-10 PBSWG = 0.1 MJSWG = 0.1153991

+CF = 0 PVTH0 = 0.0585501 PRDSW = 133.285505

+PK2 = -0.0299638 WKETA = -0.0248758 LKETA = 1.173187E-3

+AF = 1 KF = 0)

\*

.MODEL PMOS PMOS ( LEVEL = 8

+VERSION = 3.1 TNOM = 27 TOX = 1.39E-8

+XJ = 1.5E-7 NCH = 1.7E17 VTH0 = -0.9214347

+K1 = 0.5553722 K2 = 8.763328E-3 K3 = 6.3063558

+K3B = -0.6487362 W0 = 1.280703E-8 NLX = 2.593997E-8

+DVT0W = 0 DVT1W = 0 DVT2W = 0

+DVT0 = 2.5131165 DVT1 = 0.5480536 DVT2 = -0.1186489

+U0 = 212.0166131 UA = 2.807115E-9 UB = 1E-21

+UC = -5.82128E-11 VSAT = 1.713601E5 A0 = 0.8430019

+AGS = 0.1328608 B0 = 7.117912E-7 B1 = 5E-6

+KETA = -3.674859E-3 A1 = 4.77502E-5 A2 = 0.3

+RDSW = 2.837206E3 PRWG = -0.0363908 PRWB = -1.016722E-5

+WR = 1 WINT = 2.838038E-7 LINT = 5.528807E-8

+XL = 0 XW = 0 DWG = -1.606385E-8

+DWB = 2.266386E-8 VOFF = -0.0558512 NFACTOR = 0.9342488

+CIT = 0 CDSC = 2.4E-4 CDSCD = 0

+CDSCB = 0 ETA0 = 0.3251882 ETAB = -0.0580325

+DSUB = 1 PCLM = 2.2409567 PDIBLC1 = 0.0411445

+PDIBLC2 = 3.355575E-3 PDIBLCB = -0.0551797 DROUT = 0.2036901

+PSCBE1 = 6.44809E9 PSCBE2 = 6.300848E-10 PVAG = 0

+DELTA = 0.01 RSH = 101.6 MOBMOD = 1

+PRT = 59.494 UTE = -1 KT1 = -0.2942

+KT1L = 1.68E-9 KT2 = 0 UA1 = 4.5E-9

+UB1 = -6.3E-18 UC1 = -1E-10 AT = 1E3

+WL = 0 WLN = 1 WW = 0

+WWN = 1 WWL = 0 LL = 0

+LLN = 1 LW = 0 LWN = 1

+LWL = 0 CAPMOD = 2 XPART = 0.5

+CGDO = 2.9E-10 CGSO = 2.9E-10 CGBO = 1E-9

+CJ = 7.235528E-4 PB = 0.9527355 MJ = 0.4955293

+CJSW = 2.692786E-10 PBSW = 0.99 MJSW = 0.2958392

+CJSWG = 6.4E-11 PBSWG = 0.99 MJSWG = 0.2958392

+CF = 0 PVTH0 = 5.98016E-3 PRDSW = 14.8598424

+PK2 = 3.73981E-3 WKETA = 5.292165E-3 LKETA = -4.205905E-3

+AF = 1 KF = 0)